GSIC - Global Service Information Center

# DRIVE BELT > INSTALLATION

## for Preparation Click here

1. INSTALL DRIVE BELT

1. Install the drive belt to the pulleys except the drive belt tensioner pulley.

1. Use the hexagon-shaped part indicated by the arrow in the illustration to move the tensioner pulley downward and then install the drive belt to the tensioner pulley.

   NOTICE:
   1. The backside of the drive belt should face the tensioner pulley.
   2. Check that the drive belt is properly set to each pulley.

1. After a new belt has been installed, check that the tensioner indicator mark is within range A shown in the illustration.