GSIC - Global Service Information Center

# STEERING COLUMN > TORQUE SPECIFICATIONS

Part Tightened | N*m | kgf*cm | ft.*lbf
Steering wheel set nut | 50 | 510 | 37
Steering wheel pad set screw | 8.8 | 90 | 78 n.*lbf
Steering column cover upper x Steering column cover lower | 2.0 | 20 | 18 in.*lbf
Steering column assembly set nut | 21 | 214 | 15
Steering column assembly x Steering sliding w/ coupling yoke sub-assembly | 28 | 286 | 21
Steering sliding w/ coupling yoke sub-assembly x Steering sliding yoke | 35 | 355 | 26
Power steering gear box x intermediate shaft No. 2 | 35 | 355 | 26
Steering column hole cover sub-assembly x Body | 5.0 | 51 | 44 in.*lbf
Steering column clamp upper x Steering column upper w/ switch bracket assembly | 18 | 244 | 13