GSIC - Global Service Information Center

# REAR PLANETARY GEAR > DISASSEMBLY

## for Preparation Click here

1. REMOVE OUTPUT SHAFT

2. REMOVE PLANETARY OUTPUT SHAFT OIL SEAL RING

3. REMOVE REAR PLANETARY RING GEAR

4. INSPECT NO. 2 ONE-WAY CLUTCH

1. Hold the planetary gear and turn the one-way clutch inner race. Check that the one-way clutch inner race can be turned freely counterclockwise and locks when turned clockwise.

5. REMOVE NO. 2 ONE-WAY CLUTCH

1. Remove the inner race from the planetary gear.

1. Using a screwdriver, pry out the snap ring.

1. Remove the one-way clutch with the retainers from the planetary gear.

6. REMOVE NO. 2 PLANETARY CARRIER THRUST WASHER

7. REMOVE NO. 1 PLANETARY CARRIER THRUST WASHER

8. REMOVE REAR PLANETARY FLANGE THRUST NEEDLE ROLLER BEARING

1. Remove the 2 races and bearing from the planetary ring gear.

9. REMOVE REAR PLANETARY RING GEAR FLANGE

1. Using a screwdriver, pry out the snap ring.

1. Remove the ring gear flange.

10. INSPECT PLANETARY PINION GEAR THRUST CLEARANCE

1. Using a feeler gauge, measure the thrust clearance.

   Standard clearance:
     0.20 to 0.60 mm (0.0079 to 0.0236 in.)

   Maximum clearance:
     0.65 mm (0.0256 in.)
   If the clearance is greater than the maximum, replace the planetary gear.