GSIC - Global Service Information Center

# ROOM LIGHT ASSEMBLY > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE NO. 1 ROOM LIGHT LENS

1. Using a screwdriver, detach the 4 claws and remove the lens.

   HINT:
     Tape the screwdriver tip before use.

3. REMOVE NO. 1 ROOM LIGHT ASSEMBLY

1. Remove the 2 screws and room light.

1. Disconnect the lamp connector.

4. REMOVE NO. 1 ROOM LIGHT BULB

1. Remove the bulb from the room light.