GSIC - Global Service Information Center

# SPEED SENSOR > INSTALLATION

## for Preparation Click here

1. INSTALL O/D DIRECT CLUTCH SPEED SENSOR

1. Coat a new O-ring with ATF and install it to the sensor.

1. Install the sensor with the bolt.

   Torque:
     5.4 N*m{ 55 kgf*cm , 48 in.*lbf }

1. Connect the sensor connector.

2. INSTALL NO. 2 VEHICLE SPEED SENSOR

1. Coat a new O-ring with ATF and install it to the sensor.

1. Install the sensor with the bolt.

   Torque:
     5.4 N*m{ 55 kgf*cm , 48 in.*lbf }

1. Connect the sensor connector.