GSIC - Global Service Information Center

# WIRELESS DOOR LOCK CONTROL SYSTEM > REGISTRATION

1. DESCRIPTION OF CODE REGISTRATION

HINT:

1. Recognition code registration is necessary when replacing the door control transmitter or the door control receiver.
2. Add mode is used to register new recognition codes while retaining codes already registered. This mode is used when a new transmitter is added. If the number of registered codes exceeds 4, the previously registered codes will be erased in order, starting from the first registered code.
3. Rewrite mode is used to erase all previously registered recognition codes in order to register new recognition codes. This mode is used when the transmitter or the receiver is replaced.
4. Confirmation mode is used to confirm how many recognition codes have already been registered before another recognition code is registered.
5. Prohibition mode is used to erase all the registered codes and disable the wireless door lock function. This mode is used when the transmitter is lost.
6. All of the following registration procedures must be performed in order.

2. REGISTER RECOGNITION CODE

1. Check that the following conditions are met.

   1. No key in the ignition key cylinder.
   2. The driver side door is opened (the other doors are closed).

1. Insert the key into the ignition key cylinder, then pull it out twice within 5 seconds.

1. Perform the following operations within 45 seconds.

   1. Close and open the driver side door twice.

   2. Insert the key into the ignition key cylinder, then pull it out.

   3. Close and open driver side door twice.

1. Perform the following operations within 40 seconds.

   1. Perform the operation of the ignition switch according the number of times shown below.

      HINT:
        If the number of ignition switch ON-OFF operations is 0, 4, 6, or more, there will be no response (power door lock and unlock operation) to show which mode has been selected.

   2. Remove the key from the ignition key cylinder.

1. Check the response to the selected mode within 3 seconds.

   HINT:
   1. In the confirmation mode, LOCK-UNLOCK operation will occur once for each recognition code that has been registered. For example, if 2 recognition codes have been registered, the LOCK-UNLOCK operation will occur 2 times.
   2. In confirmation mode, if no recognition codes have been registered, the LOCK-UNLOCK operation will occur 5 times.
   3. If confirmation mode or prohibition mode is selected, the operation ends after the response to the selected mode completes.

1. Within 40 seconds of completing the confirmation mode operation, press the LOCK and UNLOCK switches on the transmitter simultaneously.

1. After completing the above step, press a single switch (LOCK or UNLOCK) within 5 seconds.

1. After completing the above step, check the response to the registration completion within 3 seconds.

   HINT:
   1. If the registration of the recognition code has failed, perform the registration procedures from the beginning.
   2. If registering another transmitter, repeat the procedures after the response to the selected mode confirmation. All 4 recognition codes can be registered consecutively.

1. Perform either of the following.

   1. Open the door.

   2. Insert the key into the ignition key cylinder.

1. Registration of the recognition codes (add mode and rewrite mode) is completed.