GSIC - Global Service Information Center

# MAGNETIC CLUTCH RELAY > ON-VEHICLE INSPECTION

## for Preparation Click here

1. INSPECT MAGNET CLUTCH RELAY (w/ PTC HEATER)

1. Measure the resistance of the magnet clutch relay.

   Standard resistance:

     Tester Connection | Specified Condition
     3 - 5 | 10 kΩ or higher
     3 - 5 | Below 1 Ω (when battery voltage is applied to terminals 1 and 2)

   If the result is not as specified, replace the relay.