GSIC - Global Service Information Center

# DRIVE BELT > REMOVAL

## for Preparation Click here

1. REMOVE DRIVE BELT

1. Use the hexagon-shaped part indicated by the arrow in the illustration to move the tensioner pulley downward and decrease the tension in the drive belt. Then remove the drive belt.

   NOTICE:
     When removing the drive belt, do not use the idle pulley's bolt.

   HINT:
     After removing the drive belt, move the tensioner upward to the maximum amount.