GSIC - Global Service Information Center

# 2KD-FTV INTAKE > TORQUE SPECIFICATIONS

Turbocharger:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Turbocharger sub-assembly x Exhaust manifold | 52 | 530 | 38
  Turbo oil pipe sub-assembly x Turbocharger | 13 | 133 | 10
  Turbo oil pipe sub-assembly x Turbocharger | Bolt | 12 | 122 | 9
  Union bolt | 26 | 265 | 19
  Manifold stay x Turbocharger | 19 | 194 | 14
  Manifold stay x Engine mount bracket
  Turbine outlet elbow x Turbocharger | 26 | 265 | 19
  Turbocharger stay x Turbocharger | 24 | 245 | 18
  Turbocharger stay x Cylinder block
  Air cleaner pipe sub-assembly x Intake manifold | 20 | 204 | 15
  Air cleaner pipe sub-assembly x Diesel throttle body assembly | Hose clamp | 6.5 | 66 | 58 ft.*lbf
  Air cleaner pipe sub-assembly x Turbocharger | 6.5 | 66 | 58 ft.*lbf
  Ventilation hose heat insulator x Cylinder head cover | 12 | 122 | 9
  Air cleaner assembly x Body panel | 14 | 143 | 10