GSIC - Global Service Information Center

# VACUUM SWITCHING VALVE (for EVAP) > INSTALLATION

## for Preparation Click here

1. INSTALL VACUUM SWITCHING VALVE ASSEMBLY (for EVAP)

1. Install the switching valve with the bolt.

   Torque:
     5.0 N*m{ 51 kgf*cm , 44 in.*lbf }

1. Connect the 2 hoses.

1. Connect the connector.

2. INSTALL V-BANK COVER

1. Install the cover with the 2 nuts.

   Torque:
     7.5 N*m{ 76.5 kgf*cm , 66 in.*lbf }

3. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

4. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.