GSIC - Global Service Information Center

### INTAKE MANIFOLD > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE NO. 1 ENGINE COVER SUB-ASSEMBLY

3. REMOVE CHARGE AIR COOLER ASSEMBLY WITH INTAKE AIR CONNECTOR

4. REMOVE VACUUM SWITCHING VALVE BRACKET

5. REMOVE DIESEL THROTTLE BODY ASSEMBLY

6. REMOVE THROTTLE BODY BRACKET

7. REMOVE INTAKE AIR CONNECTOR

8. REMOVE NO. 1 EGR PIPE SUB-ASSEMBLY

9. REMOVE EGR VALVE ASSEMBLY

10. REMOVE MANIFOLD STAY

11. REMOVE OIL LEVEL GAUGE GUIDE

12. REMOVE INJECTION PIPE SUB-ASSEMBLY

13. REMOVE NO. 2 NOZZLE LEAKAGE PIPE ASSEMBLY

14. REMOVE INTAKE MANIFOLD