GSIC - Global Service Information Center

# AIR FUEL RATIO SENSOR (for Unleaded Gasoline Specification Vehicle) > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE AIR FUEL RATIO SENSOR

1. Disconnect the sensor connector.

1. Detach the 3 wire clamps.

1. Using SST, remove the sensor.

   SST
     09224-00010