GSIC - Global Service Information Center

# BRAKE SYSTEM > PRECAUTION

## for Preparation Click here

NOTICE:

1. Take extra care to replace each part properly. Improper installation or repair could affect the performance of the brake system and cause a driving hazard.
2. It is very important to keep the brake system parts and the work area clean when repairing the brake system.
3. If the vehicle is equipped with a mobile communication system, refer to the Precautions in the INTRODUCTION section.
4. Care must be taken when using magnets as it could affect the performance of the speed sensors.
5. Since the brake line is one of the critical safety related parts, be sure to disassemble the components if a brake fluid leak is found. If any abnormality is found, replace the component with a new one.
6. When removing brake components, cover the brake tube connections to prevent foreign matter such as dust or dirt from entering the tubes.
7. Do not damage or deform the brake tubes when removing or installing them.
8. When installing a grommet to the body, ensure that the brake tube passes through the center of the grommet.
9. When installing a brake tube or flexible hose, ensure that they are free from twisting or bending.
10. If the cap of the flexible hose does not match the groove on the bracket, twist the hose slightly to insert it.
11. Do not reuse a clip removed from a flexible hose.
12. Flexible hoses must be free from absorber oil, grease, etc.
13. When installing a brake tube to a plastic clamp, ensure that the brake tube is not loose or being pinched.
14. Do not reuse a clip or plastic clamp removed from a flexible hose.
15. After installing a brake tube and flexible hose, ensure that they do not interfere with any other components.
16. Do not allow brake fluid to adhere to any painted surface such as the vehicle body. If brake fluid leaks onto any painted surface, immediately wash it off.

17. Follow these procedures when disconnecting and connecting the flexible hose and brake tube.

1. Remove the clip.
2. Hold the flexible hose with a wrench and disconnect the brake tube with SST without deforming the tube.
3. Connect the brake tube with a union nut wrench without deforming the tube.

1. Follow these procedures when connecting the brake tube and way.

1. Support the way to prevent deformation to the brake tube and connect the brake tube to the way with a union nut wrench.
2. Support the way to prevent deformation to the brake tube and install the bolt to fix the way to the body.