GSIC - Global Service Information Center

# FRONT DOOR COURTESY SWITCH > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the RH and LH sides.
2. The procedures listed below are for the LH side.
3. A bolt without a torque specification is shown in the standard bolt chart (Click here).

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE FRONT DOOR COURTESY LIGHT SWITCH ASSEMBLY

1. Remove the bolt and switch.

1. Disconnect the connector.