GSIC - Global Service Information Center

### RADIATOR > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE NO. 1 ENGINE UNDER COVER

3. REMOVE RADIATOR GRILLE

4. REMOVE RADIATOR SIDE DEFLECTOR LH

5. REMOVE RADIATOR SIDE DEFLECTOR RH

6. DRAIN ENGINE COOLANT

7. DISCONNECT RADIATOR HOSE INLET

8. DISCONNECT RADIATOR HOSE OUTLET

9. DISCONNECT NO. 1 OIL COOLER INLET TUBE (for Automatic Transmission)

10. DISCONNECT NO. 1 OIL COOLER OUTLET TUBE (for Automatic Transmission)

11. REMOVE FAN SHROUD

12. REMOVE RADIATOR ASSEMBLY