GSIC - Global Service Information Center

# FRONT NO. 2 SPEAKER > INSTALLATION

## for Preparation Click here

HINT:

1. Use the same procedures for the RH side and LH side.
2. The procedures listed below are for the LH side.

1. INSTALL FRONT NO. 2 SPEAKER ASSEMBLY

1. Install the speaker with the screw.

1. Connect the connector.

2. INSTALL FRONT DOOR LOWER FRAME BRACKET GARNISH LH

1. Attach the 2 clips to install the garnish.

3. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

4. PERFORM INITIALIZATION

1. Perform initialization (Click here ).

   NOTICE:
     Certain systems meed to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.