GSIC - Global Service Information Center

### VALVE CLEARANCE > ADJUSTMENT

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. LOOSEN FUEL TANK CAP ASSEMBLY

3. REMOVE INJECTION PIPE

4. REMOVE CYLINDER HEAD COVER SUB-ASSEMBLY

5. REMOVE INJECTOR ASSEMBLY

6. SET NO. 1 CYLINDER TO TDC/COMPRESSION

7. INSPECT VALVE CLEARANCE

8. ADJUST VALVE CLEARANCE

9. INSTALL INJECTOR ASSEMBLY

10. CHECK FOR FUEL LEAKS

11. INSTALL CYLINDER HEAD COVER SUB-ASSEMBLY

12. INSTALL INJECTION PIPE

13. ADD FUEL

14. TIGHTEN FUEL TANK CAP ASSEMBLY

15. BLEED AIR FROM FUEL SYSTEM

16. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

17. PERFORM INITIALIZATION

18. CHECK FOR FUEL LEAKS

19. CHECK FOR ENGINE OIL LEAKS