GSIC - Global Service Information Center

# FRONT WASHER MOTOR > INSTALLATION

## for Preparation Click here

1. INSTALL WINDSHIELD WASHER MOTOR AND PUMP ASSEMBLY

1. Install the windshield washer motor and pump to the packing of the washer jar.

2. INSTALL WINDSHIELD WASHER JAR ASSEMBLY

1. Install the windshield washer jar and pump with the clip and 3 bolts.

1. Connect the connector.

3. FILL UP WASHER JAR AND PUMP ASSEMBLY WITH WASHER FLUID

1. Connect the washer hose to the washer motor and pump, and fill the washer jar with washer fluid.

4. INSTALL FRONT FENDER LINER LH

1. Install the fender liner with the 3 clips and screw.

5. INSTALL WASHER INLET SUB-ASSEMBLY

1. Install the washer inlet of the washer jar and pump to the windshield washer jar and pump.

1. Install the washer inlet of the washer jar and pump with the clip.

6. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

7. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.