GSIC - Global Service Information Center

# HIGH MOUNTED STOP LIGHT ASSEMBLY > INSTALLATION

## for Preparation Click here

1. INSTALL CENTER STOP LIGHT ASSEMBLY

1. Attach the center stop light with the 4 claws.

1. Connect the connector.

2. INSTALL TAIL GATE SERVICE HOLE COVER

1. Using a T30 "torx" socket, install the 10 screws and cover.

3. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

4. PERFORM INITIALIZATION

1. Perform initialization (Click here ).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.