GSIC - Global Service Information Center

### GLOW PLUG > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE ENGINE COVER SUB-ASSEMBLY

3. REMOVE CHARGE AIR COOLER ASSEMBLY

4. REMOVE VACUUM SWITCHING VALVE BRACKET

5. REMOVE DIESEL THROTTLE BODY ASSEMBLY

6. REMOVE THROTTLE BODY BRACKET

7. REMOVE INTAKE AIR CONNECTOR

8. REMOVE NO. 1 EGR PIPE SUB-ASSEMBLY

9. REMOVE EGR VALVE ASSEMBLY

10. REMOVE NO. 1 GLOW PLUG CONNECTOR

11. REMOVE GLOW PLUG ASSEMBLY