GSIC - Global Service Information Center

### COMMON RAIL > INSTALLATION

1. INSTALL COMMON RAIL ASSEMBLY

2. INSTALL FUEL INLET PIPE SUB-ASSEMBLY

3. INSTALL NO. 2 NOZZLE LEAKAGE PIPE ASSEMBLY

4. INSTALL INJECTION PIPE

5. INSTALL OIL FILTER SUB-ASSEMBLY

6. INSTALL MANIFOLD STAY

7. INSTALL CHARGE AIR COOLER ASSEMBLY WITH INTAKE AIR CONNECTOR

8. INSTALL NO. 1 ENGINE COVER SUB-ASSEMBLY

9. ADD FUEL

10. TIGHTEN FUEL TANK CAP ASSEMBLY

11. ADD ENGINE OIL

12. BLEED AIR FROM FUEL SYSTEM

13. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

14. PERFORM INITIALIZATION

15. CHECK FOR ENGINE OIL LEAKS

16. CHECK FOR FUEL LEAKS

17. INSTALL NO. 2 ENGINE UNDER COVER (for 4WD)

18. INSTALL NO. 1 ENGINE UNDER COVER (for 4WD)