GSIC - Global Service Information Center

### EXHAUST PIPE > INSTALLATION

1. INSTALL FRONT EXHAUST PIPE ASSEMBLY

2. INSTALL FRONT NO. 2 EXHAUST PIPE ASSEMBLY

3. INSTALL CENTER EXHAUST PIPE ASSEMBLY

4. INSTALL TAILPIPE ASSEMBLY

5. INSTALL HEATED OXYGEN SENSOR (for Bank 1 Sensor 2)

6. INSTALL HEATED OXYGEN SENSOR (for Bank 2 Sensor 2)

7. CONNECT CABLE TO BATTERY NEGATIVE TERMINAL

8. CHECK EXHAUST GAS LEAKS

9. PERFORM INITIALIZATION