GSIC - Global Service Information Center

# THROTTLE BODY > INSTALLATION

## for Preparation Click here

1. INSTALL THROTTLE BODY

1. Install a new gasket to the intake air surge tank.

1. Install the throttle motor connector.

   Torque:
     11 N*m{ 112 kgf*cm , 9 ft.*lbf }

2. REMOVE AIR CLEANER ASSEMBLY

Torque:
  8.0 N*m{ 82 kgf*cm , 71 in.*lbf }

3. REMOVE NO. 2 VENTILATION HOSE

4. REMOVE V-BANK COVER

Torque:
  7.5 N*m{ 76 kgf*cm , 66 in.*lbf }

5. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

6. ADD ENGINE COOLANT

1. Tighten all the plugs and fill the radiator with TOYOTA Super Long Life Coolant (SLLC).

   Torque:
     24.5 N*m{ 250 kgf*cm , 18 ft.*lbf } for cylinder block drain cock plug

   Standard capacity:

     Item | Specified Condition
     A/T | 9.8 liters (10.4 US qts, 8.6 lmp. qts)
     M/T | 8.5 liters (9.0 US qts, 7.5 lmp. qts)

   HINT:
   1. TOYOTA vehicles are filled with TOYOTA SLLC at the factory. In order to avoid damage to the engine cooling system and other technical problems, only use TOYOTA SLLC or similar high quality ethylene glycol based non-silicate, non-amine, non-nitrite, non-borate coolant with long-life hybrid organic acid technology (coolant with long-life hybrid organic and technology consists of a combination of low phosphates and organic acids).
   2. Please contact your TOYOTA dealer for further details.

   NOTICE:
     Never use water as a substitute for engine coolant.

1. Press the inlet and outlet radiator hoses several times by hand, and then check the level of the coolant.

1. Install the radiator cap.

1. Bleed air from the cooling system.

   1. Warm up the engine until the thermostat opens. While the thermostat is open, circulate the coolant for several minutes.

   2. Maintain the engine speed at 2,000 to 2,500 rpm.

   3. Press the inlet and outlet radiator hoses several times by hand to bleed air.

      CAUTION:
      When pressing the radiator hoses:
      1. Wear protective gloves.
      2. Be careful as the radiator hoses are hot.
      3. Keep your hands away from the radiator fan.

1. Stop the engine and wait until the coolant cools down to ambient temperature.

   CAUTION:
     Do not remove the radiator cap while the engine and radiator are still hot. Pressurized, hot engine coolant and steam may be released and cause serious burns.

1. Check the coolant level in the radiator reservoir.
   If the coolant level is low, add SLLC to the reservoir F line.

7. CHECK FOR ENGINE COOLANT LEAKS

1. Check for engine coolant leaks (Click here).

8. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.