GSIC - Global Service Information Center

# GENERATOR > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretentioner activation.

2. REMOVE V-BANK COVER

1. Remove the 2 nuts and cover.

3. REMOVE DRIVE BELT

1. While releasing the belt tension by turning the belt tensioner counterclockwise, remove the V-ribbed belt from the belt tensioner.

4. REMOVE GENERATOR ASSEMBLY

1. Remove the nut and generator wire.

1. Disconnect the generator connector.

1. Remove the 2 bolts, adjusting bar and generator.