GSIC - Global Service Information Center

# FRONT PROPELLER SHAFT ASSEMBLY > INSTALLATION

## for Preparation Click here

1. INSTALL FRONT PROPELLER SHAFT ASSEMBLY

1. Align the matchmarks on the yoke and differential flange.

1. Connect the propeller shaft with the 4 bolts, 4 nuts and 4 washers.

   Torque:
     88 N*m{ 897 kgf*cm , 65 ft.*lbf }

1. Align the matchmarks on the yoke and transfer flange.

   Torque:
     88 N*m{ 897 kgf*cm , 65 ft.*lbf }