GSIC - Global Service Information Center

### TURBOCHARGER > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. DRAIN ENGINE COOLANT

3. REMOVE FRONT WHEEL RH

4. REMOVE FRONT FENDER APRON SEAL UPPER

5. REMOVE FRONT FENDER SEAL

6. REMOVE FRONT EXHAUST PIPE ASSEMBLY

7. REMOVE AIR CLEANER ASSEMBLY

8. REMOVE NO. 1 ENGINE COVER SUB-ASSEMBLY

9. REMOVE CHARGE AIR COOLER ASSEMBLY WITH INTAKE AIR CONNECTOR

10. REMOVE COMPRESSOR INLET ELBOW

11. REMOVE NO. 1 EXHAUST MANIFOLD HEAT INSULATOR

12. REMOVE NO. 1 TURBO INSULATOR

13. REMOVE NO. 1 TURBO WATER HOSE

14. REMOVE TURBINE OUTLET ELBOW

15. REMOVE TURBOCHARGER STAY

16. REMOVE TURBO OIL INLET PIPE SUB-ASSEMBLY

17. REMOVE TURBOCHARGER SUB-ASSEMBLY