GSIC - Global Service Information Center

# INTAKE AIR TEMPERATURE SENSOR > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE ENGINE COVER SUB-ASSEMBLY

1. Remove the 3 bolts, 2 nuts and cover.

3. REMOVE INTAKE AIR TEMPERATURE SENSOR

1. Disconnect the IAT sensor connector.

1. Using a 22 mm deep socket wrench, remove the IAT sensor.

   HINT:
     Replace the IAT sensor if it is deformed, cracked or malfunctioning. It is not necessary to replace the IAT sensor each time the CAC is replaced.