GSIC - Global Service Information Center

# ROOF HEADLINING (for Double Cab) > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE FRONT DOOR SCUFF PLATE LH

1. Using a screwdriver, detach the 7 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 3 clips and remove the scuff plate.

3. REMOVE FRONT DOOR SCUFF PLATE RH

HINT:

  Use the same procedures described for the LH side.

4. REMOVE FRONT DOOR OPENING TRIM LH

5. REMOVE FRONT DOOR OPENING TRIM RH

6. REMOVE COWL SIDE TRIM BOARD LH

1. Remove the cap nut.

1. Using a clip remover, detach the 2 clips and remove the trim board.

7. REMOVE COWL SIDE TRIM BOARD RH

HINT:

  Use the same procedures described for the LH side.

8. REMOVE REAR DOOR SCUFF PLATE LH

1. Using a screwdriver, detach the 7 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 2 clips and remove the scuff plate.

9. REMOVE REAR DOOR SCUFF PLATE RH

HINT:

  Use the same procedures described for the LH side.

10. REMOVE REAR DOOR OPENING TRIM WEATHERSTRIP LH

11. REMOVE REAR DOOR OPENING TRIM WEATHERSTRIP RH

12. REMOVE FRONT SEAT OUTER BELT ASSEMBLY LH

1. Single cab:
   Remove the outer belt shoulder anchor.

   1. Using a screwdriver, detach the 2 claws and open the seat belt anchor cover.

      HINT:
        Tape the screwdriver tip before use.

   2. Remove the bolt and shoulder anchor.

1. Double cab:
   Remove the outer belt shoulder anchor.

   1. Using a screwdriver, disengage the 4 claws and remove the seat belt anchor cover cap.

      HINT:
        Tape the screwdriver tip before use.

   2. Remove the bolt and shoulder anchor.

1. w/o Pretensioner:
   Remove the bolt and seat belt.

1. w/ Pretensioner:

   1. Disconnect the pretensioner connector as shown in the illustration.

   2. Remove the bolt and seat belt.

13. REMOVE FRONT SEAT OUTER BELT ASSEMBLY RH

1. Single cab:
   Remove the outer belt shoulder anchor.

   1. Using a screwdriver, detach the 2 claws and open the seat belt anchor cover.

      HINT:
        Tape the screwdriver tip before use.

   2. Remove the bolt and shoulder anchor.

1. Double cab:
   Remove the outer belt shoulder anchor.

   1. Using a screwdriver, disengage the 4 claws and remove the seat belt anchor cover cap.

      HINT:
        Tape the screwdriver tip before use.

   2. Remove the bolt and shoulder anchor.

1. w/o Pretensioner:
   Remove the bolt and seat belt.

1. w/ Pretensioner:

   1. Disconnect the pretensioner connector as shown in the illustration.

   2. Remove the bolt and seat belt.

14. REMOVE CENTER PILLAR GARNISH LOWER LH

1. Using a screwdriver, detach the 2 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 2 clips and remove the garnish.

15. REMOVE CENTER PILLAR GARNISH LOWER RH

HINT:

  Use the same procedures described for the LH side.

16. REMOVE CENTER PILLAR GARNISH LH

1. Using a clip remover, detach the clip.

1. Pull the garnish in the direction indicated by the arrow in the illustration to detach the claw. Then remove the garnish.

17. REMOVE CENTER PILLAR GARNISH RH

HINT:

  Use the same procedures described for the LH side.

18. REMOVE FRONT PILLAR GARNISH LH

1. w/ Assist grip:
   Using a screwdriver, detach the 4 claws and pry out the 2 assist grip plugs.

   HINT:
     Tape the screwdriver tip before use.

1. w/ Assist grip:
   Remove the 2 screws and the assist grip.

1. Using a clip remover, detach the 2 clips.

1. Pull the garnish in the direction indicated by the arrow in the illustration to detach the 2 claws. Then remove the garnish.

19. REMOVE FRONT PILLAR GARNISH RH

HINT:

  Use the same procedures described for the LH side.

20. REMOVE BACK PANEL GARNISH UPPER

1. Using a screwdriver, detach the 4 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 5 clips and remove the garnish.

21. REMOVE BACK PANEL TRIM (w/ Back Panel Trim)

1. Using a clip remover, remove the 3 clips and remove the back panel trim.

22. REMOVE QUARTER TRIM PANEL LOWER LH

1. Using a screwdriver, detach the claw.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 3 clips and remove the trim panel.

23. REMOVE QUARTER TRIM PANEL LOWER RH

HINT:

  Use the same procedures described for the LH side.

24. REMOVE REAR NO. 1 SEAT BELT ASSEMBLY OUTER LH

1. Remove the bolt and floor anchor.

1. Using a screwdriver, detach the 2 claws and open the seat belt anchor cover.

   HINT:
     Tape the screwdriver tip before use.

1. Remove the bolt.

1. Remove the bolt and seat belt.

25. REMOVE REAR NO. 1 SEAT BELT ASSEMBLY OUTER RH

1. Remove the bolt and floor anchor.

1. Using a screwdriver, detach the 2 claws and open the seat belt anchor cover.

   HINT:
     Tape the screwdriver tip before use.

1. Remove the bolt.

1. Remove the bolt and seat belt.

26. REMOVE QUARTER INSIDE TRIM BOARD LH

1. Using a clip remover, detach the 4 clips and remove the trim board.

27. REMOVE QUARTER INSIDE TRIM BOARD RH

HINT:

  Use the same procedures described for the LH side.

28. REMOVE ROOM LIGHT ASSEMBLY

Click here

29. REMOVE VISOR ASSEMBLY LH

1. Remove the 2 screws and visor.

30. REMOVE VISOR ASSEMBLY RH

1. Remove the 2 screws and visor.

31. REMOVE VISOR HOLDER LH

1. Remove the screw.

1. Using a screwdriver, detach the 2 claws and remove the holder.

   HINT:
     Tape the screwdriver tip before use.

32. REMOVE VISOR HOLDER RH

HINT:

  Use the same procedures described for the LH side.

33. REMOVE ASSIST GRIP

1. w/o Rear roof assist grip:
   Using a screwdriver, detach the 4 claws and open the 2 covers.

   HINT:
     Tape the screwdriver tip before use.

1. w/o Rear roof assist grip:
   Remove the 2 screws and assist grip.

1. w/ Rear roof assist grip:
   Using a screwdriver, detach the 12 claws and open the 6 covers.

   HINT:
     Tape the screwdriver tip before use.

1. w/ Rear roof assist grip:
   Remove the 6 screws and 3 assist grips.

34. REMOVE ROOF HEADLINING ASSEMBLY

1. w/o Rear roof assist grip:
   Using a clip remover, remove the 9 clips and headlining.

1. w/ Rear roof assist grip:
   Using a clip remover, remove the 5 clips and headlining.

1. Remove the wire harness.

35. REMOVE ROOF NO. 2 SILENCER PAD

1. Remove the 2 silencer pads.

36. REMOVE SIDE RAIL SPACER FRONT LH

37. REMOVE SIDE RAIL SPACER FRONT RH

38. REMOVE SIDE RAIL SPACER REAR LH

1. LHD, w/o Rear roof assist grip:
   Remove the 2 spacers.

1. LHD, w/ Rear roof assist grip:
   Remove the spacer.

1. RHD, w/o Rear roof assist grip:
   Remove the spacer.

39. REMOVE SIDE RAIL SPACER REAR RH

1. LHD, w/o Rear roof assist grip:
   Remove the spacer.

1. RHD, w/o Rear roof assist grip:
   Remove the 2 spacers.

1. RHD, w/ Rear roof assist grip:
   Remove the spacer.

40. REMOVE NO. 2 SIDE RAIL SPACER REAR LH

1. Remove the 2 spacers.

41. REMOVE NO. 2 SIDE RAIL SPACER REAR RH

1. Remove the 2 spacers.

42. REMOVE NO. 3 SIDE RAIL SPACER REAR LH

43. REMOVE NO. 3 SIDE RAIL SPACER REAR RH