GSIC - Global Service Information Center

# REAR LEAF SPRING (for 4WD) > DISASSEMBLY

## for Preparation Click here

1. REMOVE REAR LEAF SPRING SHACKLE LOWER BUSH

1. Using a screwdriver, remove the 2 bushes from the spring shackle side or spring side.

   HINT:
     Tape the screwdriver tip before use.

2. REMOVE REAR LEAF SPRING SHACKLE UPPER BUSH

1. Using a screwdriver, remove the 2 bushes from the spring shackle side or spring side.

   HINT:
     Tape the screwdriver tip before use.