GSIC - Global Service Information Center

### DIFFERENTIAL VACUUM ACTUATOR > REPLACEMENT

1. REMOVE FRONT SIDE MEMBER TO FRONT SUSPENSION CROSSMEMBER BRACE

2. REMOVE NO. 1 ENGINE UNDER COVER

3. REMOVE NO. 2 ENGINE UNDER COVER

4. DRAIN DIFFERENTIAL OIL

5. REMOVE DIFFERENTIAL VACUUM ACTUATOR ASSEMBLY

6. INSTALL DIFFERENTIAL VACUUM ACTUATOR ASSEMBLY

7. REFILL DIFFERENTIAL OIL

8. CHECK FOR DIFFERENTIAL OIL LEAKAGE

9. INSTALL NO. 2 ENGINE UNDER COVER

10. INSTALL NO. 1 ENGINE UNDER COVER

11. INSTALL FRONT SIDE MEMBER TO FRONT SUSPENSION CROSSMEMBER BRACE