GSIC - Global Service Information Center

# FRONT SEAT INNER BELT ASSEMBLY > INSPECTION

## for Preparation Click here

1. INSPECT FRONT SEAT INNER BELT ASSEMBLY (for Driver Side)

1. Measure the resistance of the buckle switch.

   Standard resistance:

     Tester Connection | Condition | Specified Condition
     1 - 2 | Seat belt is unfastened | Below 1 Ω
     1 - 2 | Seat belt is fastened | 1 MΩ or higher

   If the result is not as specified, replace the belt assembly.

2. INSPECT OCCUPANT DETECTION SENSOR

1. Measure the resistance of the sensor.

   Standard:

     Condition | Specified Condition
     Apply more than 29 N (3 kgf, 7 lbf) to occupant detection sensor | 100 Ω or lower
     Seat not occupied | 1 MΩ or higher

   If the result is not as specified, replace the belt assembly.

3. INSPECT FRONT SEAT INNER BELT ASSEMBLY (Passenger Side)

1. Measure the resistance of the buckle switch.

   HINT:
     Before performing the buckle switch check, perform the previous step (inspect occupant detection sensor) to make sure the occupant detection sensor is functioning normally.

   Standard resistance:

     Tester Connection | Condition | Specified Condition
     1 - 2 | Seat belt is unfastened (Apply more than 147 N (15 kgf, 33 lbf) to occupant detection sensor) | 100 Ω or lower (Below 100 Ω)
     1 - 2 | Seat belt is fastened (Apply more than 147 N (15 kgf, 33 lbf) to occupant detection sensor) | 1 MΩ or higher

   If the result is not as specified, replace the inner belt assembly.

4. INSPECT PASSENGER SEAT BELT WARNING LIGHT ASSEMBLY

1. Check the illumination area of the seat belt warning light.

   OK:

     Measurement Condition | Specified Condition
     Battery positive (+) → 3 (IG) Battery negative (-) → 2 (SW), 1(GND) | Illuminates

   If the result is not as specified, replace the inner belt assembly.