GSIC - Global Service Information Center

# AXLE > TORQUE SPECIFICATIONS

Part Tightened | N*m | kgf*cm | ft.*lbf
Front axle hub assembly x Lock nut (2WD) | 199 | 2,029 | 147
Front axle hub assembly x Hub nut (4WD) | 235 | 2,396 | 173
Steering knuckle x Tie rod end (2WD) | 49 | 500 | 36
Steering knuckle x Tie rod end (4WD) | 91 | 928 | 67
Steering knuckle x Stabilizer link (4WD) | 70 | 714 | 52
Disc brake caliper x Steering knuckle (2WD) | 126 | 1,285 | 93
Disc brake caliper x Steering knuckle (4WD) | 123 | 1,254 | 91
Disc brake caliper x Brake hose (2WD) | 29 | 296 | 21
Disc brake caliper x Brake tube (4WD) | With SST: 14 | With SST: 143 | With SST: 10
With out SST: 15 | With out SST: 155 | With out SST: 11
Front brake tube bracket set bolt (4WD) | 29 | 296 | 21
Front ABS speed sensor wire harness bracket set bolt | 13 | 133 | 10
Front ABS speed sensor set bolt | 8.0 | 82 | 71 in.*lbf
Steering knuckle x Upper ball joint | 110 | 1,122 | 81
Steering knuckle x Lower arm assembly w/ attachment LH (2WD) | 160 | 1,632 | 118
Steering knuckle x Lower arm assembly w/ attachment (4WD) | 160 | 1,632 | 118
Steering knuckle x Front axle w/ABS rotor bearing assembly (4WD) | 80 | 816 | 59
Steering knuckle x Dust cover (2WD) | 8.0 | 133 | 71 in.*lbf
Front wheel (2WD) | Steel type: 152 Aluminum type: 132 | Steel type: 1,550 Aluminum type: 1,346 | Steel type: 112 Aluminum type: 97
Front wheel (4WD) | 105 | 1,071 | 77
Rear axle housing x Rear axle shaft w/ baking plate | 68 | 700 | 50
Rear ABS speed sensor set bolt | 8.0 | 82 | 71 in.*lbf
Rear brake tube x Wheel cylinder | 15 | 155 | 11
Parking brake cable set bolt | 9.3 | 95 | 82 in.*lbf
Rear wheel (2WD) | Steel type: 152 | Steel type: 1,550 | Steel type: 112
Aluminum type: 121 | Aluminum type: 1,234 | Aluminum type: 89
Rear wheel (4WD) | 105 | 1,071 | 77