GSIC - Global Service Information Center

# PARK / NEUTRAL POSITION SWITCH > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. DISCONNECT PARK/NEUTRAL POSITION SWITCH CONNECTOR

3. REMOVE PARK/NEUTRAL POSITION SWITCH ASSEMBLY

1. Using a screwdriver, pry out the lock washer.

1. Remove the lock nut and lock washer.

1. Remove the bolt and park/neutral position switch.