GSIC - Global Service Information Center

# 1KD-FTV FUEL > TORQUE SPECIFICATIONS

Part Tightened | N*m | kgf*cm | ft.*lbf
Engine cover bracket x Cylinder head cover | 18 | 184 | 13
Cylinder head cover sub-assembly x Cylinder head | 9.0 | 92 | 80 in.*lbf
Nozzle holder clamp x Cylinder head | 22 | 220 | 16
Nozzle leakage pipe assembly x Injector assembly | Hollow screw | 16 | 163 | 12
Union bolt | 12.5 | 127 | 9.0
Fuel pipe x Injector and Common rail | 35 | 357 | 26
Fuel inlet pipe x Common rail and supply pump | 35 | 357 | 26
Fuel pipe clamp No. 2 x Fuel pipe | 5.0 | 51 | 44 in.*lbf
Fuel pipe clamp No. 3 x Fuel pipe | 5.0 | 51 | 44 in.*lbf
Nozzle leakage pipe assembly No. 2 x Cylinder head | SST (check valve) | 21 | 214 | 16
Air cleaner assembly x Body | 14 | 143 | 10
Radiator reservoir x Radiator assembly | 5.0 | 51 | 44 in.*lbf
Oil reservoir x Body | 5.0 | 51 | 44 in.*lbf
Fan shroud x Body | 5.0 | 51 | 44 in.*lbf
Cooling fan x Water pump assembly | 18 | 184 | 13 in.*lbf
Supply pump x Supply pump gear set nut | 64 | 653 | 47
Supply pump x Timing gear case | 21 | 214 | 16
Camshaft timing pulley flange No. 2 x Pump drive shaft pulley | 31 | 316 | 23
Timing belt tensioner x Timing gear case | 13 | 133 | 10
Timing belt No. 1 cover x Timing belt No. 2 cover | 6.0 | 61 | 53 in.*lbf
Oil level gage guide x Intake manifold | 8.0 | 82 | 71 in.*lbf
Clamp x Fuel inlet pipe | 5.0 | 51 | 44 in.*lbf
Common rail assembly x Cylinder block | 38 | 387 | 28
Nozzle leakage pipe assembly No. 2 x Cylinder head | Check valve | 21 | 214 | 16
Bolt | 13 | 133 | 10
Fuel tank filler pipe sub-assembly x Body | 19 | 194 | 14
Fuel tank vent tube sub-assembly x Fuel tank assembly | 1.5 | 15 | 13 in.*lbf
Fuel tank band sub-assembly No. 1 x Body | 61 | 622 | 45
Fuel tank band sub-assembly No. 1 LH x Body | 61 | 622 | 45