GSIC - Global Service Information Center

# WINDSHIELD / WINDOWGLASS > TORQUE SPECIFICATIONS

Part Tightened | N*m | kgf*cm | ft.*lbf
Wiper arm x Wiper link | 7.5 | 77 | 66 in.*lbf
Single cab Front seat outer belt assembly (shoulder anchor) x body | 42 | 428 | 31
Extra cab front seat outer belt assembly (shoulder anchor) x Front shoulder belt anchor adjuster assembly | 42 | 428 | 31
Front seat outer belt assembly (floor anchor) x Body | 42 | 428 | 31
Extra cab and double cab rear seat outer belt assembly (floor anchor) x Body | 42 | 428 | 31
Extra cab rear seat outer belt assembly (Upper part of retractor) x Body | 4.8 | 49 | 42 in.*lbf
Extra cab and double cab rear seat outer belt assembly (shoulder anchor) x body | 42 | 428 | 31
Front seat assembly x Body | 37 | 377 | 27
Extra cab rear seat back assembly x Body | 39 | 398 | 29
Double cab rear seat assembly x body | 19.5 | 199 | 14
Quarter window lock assembly x Body | 5.0 | 51 | 44 in.*lbf