GSIC - Global Service Information Center

# AIR PUMP (for Unleaded Gasoline Specification Vehicle) > INSTALLATION

## for Preparation Click here

1. INSTALL AIR PUMP ASSEMBLY

1. Install the pump to the bracket with air pump insulator.

2. CONNECT NO. 3 AIR HOSE

1. Connect the No. 3 hose to the pump.

3. CONNECT NO. 2 AIR HOSE

1. Connect the No. 2 hose to the pump.

1. Secure the No. 2 hose with the clamp.

1. Clamp the No. 2 hose and wire harness with the clamp.

4. INSTALL AIR PUMP COVER

1. Install the cover to the bracket with the 3 clips.

5. INSTALL AIR PUMP PIPE

1. Install the inlet pipe to the body panel with the bolt.

   Torque:
     13 N*m{ 133 kgf*cm , 10 ft.*lbf }

6. INSTALL AIR PUMP ASSEMBLY WITH BRACKET

1. Install the pump with bracket to the body panel with the 3 bolts.

   Torque:
     13 N*m{ 133 kgf*cm , 10 ft.*lbf }

   HINT:
     Attach the bracket's protrusion to the body's hole.

1. Connect the No. 2 and No. 3 hoses to the inlet pipe.

   HINT:
     Connect the No. 2 air hose to the pipe connected to the air switching valve.

1. Secure the No. 2 hose with the clamp.

1. Install the 2 claws to the inlet pipe and body panel.

1. Connect the connector.

7. INSTALL FRONT FENDER APRON SEAL UPPER

1. Install the apron seal with the 6 clips.

8. CONNECT NO. 4 AIR HOSE

1. Connect the No. 4 hose to the air switching valve and inlet pipe.

1. Secure the hose with the 2 clamps.

1. Clamp the hose with the clamp.

9. INSTALL AIR PUMP INLET

1. Connect the hose to the inlet pipe.

1. Install the pump inlet to the radiator tank upper with the bolt.

   Torque:
     8.5 N*m{ 87 kgf*cm , 75 in.*lbf }

10. INSTALL AIR CLEANER ASSEMBLY

1. Connect the air cleaner hose.

1. Install the air cleaner with the 2 bolts.

   Torque:
     14 N*m{ 143 kgf*cm , 10 ft.*lbf }

1. Tighten the hose clamp.

   Torque:
     4.0 N*m{ 41 kgf*cm , 35 in.*lbf }

1. Connect the MAF meter connector.

11. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

12. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   CAUTION:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.