GSIC - Global Service Information Center

# SPEED SENSOR > INSTALLATION

## for Preparation Click here

1. INSTALL VEHICLE SPEED SENSOR

1. Coat a new O-ring with ATF and install it to the sensor.

1. Install the sensor with the bolt.

   Torque:
     5.4 N*m{ 5 kgf*cm , 48 in.*lbf }

1. Connect the sensor connector

2. INSTALL SPEEDOMETER SENSOR

1. Coat a new O-ring with ATF and install it to the sensor.

1. Install the speedometer driven gear to the sensor.

   HINT:
     Install the gear so that the gear's grooves align with the protrusions inside the sensor.

1. Install the sensor assembly with the bolt.

   Torque:
     9.8 N*m{ 99 kgf*cm , 87 in.*lbf }

1. Connect the sensor connector.