GSIC - Global Service Information Center

# CIGARETTE LIGHTER > INSTALLATION

1. INSTALL CIGARETTE LIGHTER ASSEMBLY

1. Align the protrusion on the backside of the socket with the groove of the cover. Then push the socket into the cover.

2. INSTALL CIGARETTE LIGHTER COVER

1. Attach the 2 claws to install the cigarette lighter cover.

1. Connect the connector.

3. INSTALL SWITCH BASE

1. Connect all connectors.

1. Attach the 8 claws to install the switch base.

4. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

5. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.