GSIC - Global Service Information Center

# ENGINE HOOD / DOOR > TORQUE SPECIFICATIONS

HOOD
Part Tightened | N*m | kgf*cm | ft.*lbf
Hood x Hood hinge | 13 | 134 | 9.6
Hood lock x Body panel | 8.0 | 82 | 71 in.*lbf

FRONT DOOR
Part Tightened | N*m | kgf*cm | ft.*lbf
Door check x Body | 30 | 306 | 22
Door check x Door panel | 5.5 | 56 | 49 in.*lbf
Door frame sub-assembly rear lower x Door panel | 8.0 | 82 | 71 in.*lbf
Door glass x Front door regulator sub-assembly | 8.0 | 82 | 71 in.*lbf
Door hinge x Body | 26 | 265 | 19
Door hinge x Door panel | 26 | 265 | 19
Door lock x Door panel | 5.0 | 51 | 44 in.*lbf
Door lock striker x Body | 23 | 235 | 17
Door outside handle cover x Door panel | 4.0 | 41 | 35 in.*lbf
Door outside handle frame x Door panel | 4.0 | 41 | 35 in.*lbf
Power window regulator x Door panel | 5.4 | 55 | 48 in.*lbf
Window regulator x x Door panel | 8.0 | 82 | 71 in.*lbf

REAR DOOR
Part Tightened | N*m | kgf*cm | kgf*cm
Door check x Body | 30 | 306 | 22
Door check x Door panel | 5.5 | 56 | 49 in.*lbf
Door frame sub-assembly x Door panel | 8.0 | 82 | 71 in.*lbf
Door hinge x Body | 26 | 265 | 19
Door hinge x Door panel | 26 | 265 | 19
Door lock x Door panel | 5.0 | 51 | 44 in.*lbf
Door lock striker x Body | 23 | 235 | 14
Door outside handle cover x Door panel | 4.0 | 41 | 35 in.*lbf
Door outside handle frame x Door panel | 4.0 | 41 | 35 in.*lbf
Power window regulator motor x Window regulator | 5.4 | 55 | 48 in.*lbf
Window regulator x Door panel | 8.0 | 82 | 71 in.*lbf

TAIL GATE
Part Tightened | N*m | kgf*cm | kgf*cm
Tail gate handle x Door panel | 5.0 | 51 | 44 in.*lbf
Tail gate hinge x Body | 59 | 601 | 44
Tail gate hinge x Door panel | Bottom | 18 | 184 | 13
Side | 28 | 286 | 21
Tail gate lock x Door panel | 12.5 | 128 | 9.0
Tail gate lock striker x Body | 28 | 286 | 21
Tail gate stay x Body | 27 | 275 | 20
Tail gate stay x Door panel | 27 | 275 | 20