GSIC - Global Service Information Center

# POWER STEERING > SERVICE DATA

Power steering fluid | Fluid level rise | Maximum | 5 mm (0.20 in.)
Fluid pressure at idle speed with valve closed | 8.800 kPa (89.7 kgf/cm2, 1,276 psi)
Steering wheel | Steering effort at idle speed | Reference | 5.5 N*m (56 kgf*cm, 49 in.*lbf)
Power steering vane pump | Vane pump rotating torque | 0.27 N*m (2.8 kgf*cm, 2.4 in.*lbf) or less
Vane plate height | Minimum | 7.6 mm (0.299 in.)
Vane plate thickness | Minimum | 1.405 mm (0.0553 in.)
Vane plate length | Minimum | 11.993 mm (0.4722 in.)
Clearance between the rotor groove and plate | Maximum | 0.025 mm (0.0010 in.)
Spring free length | Minimum | 29.2 mm (1.150 in.)
Power steering link (2WD) | Total preload (tie rod rotating torque) | Turning | 0.29 to 1.96 N*m (2.9 to 20.0 kgf*cm, 2.57 to 17.35 in.*lbf)
Total preload (control valve rotating torque) | Turning | 0.8 to 1.6 N*m (8.2 to 16.3 kgf*cm, 7.1to 14.2 in.*lbf)
Power steering link (4WD) | Total preload (tie rod rotating torque) | Turning | 0.5 to 3.5N*m (5.1 to 35.7 kgf*cm, 0.37 to 2.58 in.*lbf)
Total preload (control valve rotating torque) | Turning | 1.0 to 1.8 N*m (10.2 to 18.4 kgf*cm, 8.9 to 15.9 in.*lbf)