GSIC - Global Service Information Center

# VENTILATION VALVE > INSTALLATION

## for Preparation Click here

1. INSTALL VENTILATION VALVE SUB-ASSEMBLY

1. Apply adhesive to 2 or 3 threads of the valve.

   Adhesive:
     Part No. 08833-00070, THREE BOND 1342 or equivalent

1. Install the valve.

   Torque:
     5.0 N*m{ 51 kgf*cm , 44 in.*lbf }

1. Connect the ventilation hose to the valve.

1. Secure the hose with the clamp.

2. INSTALL INTAKE AIR SURGE TANK

1. Install a new gasket and the surge tank with the 2 nuts.

   Torque:
     28 N*m{ 286 kgf*cm , 21 ft.*lbf }

1. Using an 8 hexagon wrench, install the 4 bolts.

   Torque:
     28 N*m{ 286 kgf*cm , 21 ft.*lbf }

1. Install the 3 upper bolts which are used to secure the 2 surge tank stays and throttle body bracket.

   Torque:
     21 N*m{ 214 kgf*cm , 16 ft.*lbf }

1. Install the 3 wire harness clamps and hose clamp.

1. Connect the throttle motor connector.

1. Connect the 2 VSV connectors.

1. Connect the ventilation hose.

1. Connect the vapor feed hose assembly.

1. Connect the No. 4 water by-pass hose.

1. Connect the No. 5 water by-pass hose.

3. INSTALL V-BANK COVER

1. Install the cover with the 2 nuts.

   Torque:
     7.5 N*m{ 76.5 kgf*cm , 66 in.*lbf }

4. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

5. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.