GSIC - Global Service Information Center

# REAR BUMPER (for Step Type) > INSTALLATION

## for Preparation Click here

1. INSTALL REAR BUMPER ARM LH

1. Install the bumper arm with the 2 bolts.

   Torque:
     45 N*m{ 459 kgf*cm , 33 ft.*lbf }

2. INSTALL REAR BUMPER ARM RH

1. Install the bumper arm with the 2 bolts.

   Torque:
     45 N*m{ 459 kgf*cm , 33 ft.*lbf }

3. INSTALL REAR BUMPER BAR

1. Install the bumper bar with the 4 bolts.

   Torque:
     45 N*m{ 459 kgf*cm , 33 ft.*lbf }