GSIC - Global Service Information Center

# REAR SPEED SENSOR > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the LH side and RH side.
2. The procedures listed below are for the LH side.

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE REAR WHEEL

3. REMOVE REAR SPEED SENSOR LH

1. Disconnect the sensor connector.

1. Remove the bolt and sensor.

   NOTICE:
     Keep the sensor tip and sensor installation hole free from foreign matter.