GSIC - Global Service Information Center

# STARTER > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag activation.

2. REMOVE FRONT FENDER SEAL

1. Remove the 5 clips and seal.

3. REMOVE STARTER ASSEMBLY

1. Disconnect the starter connector.

1. Remove the nut and disconnect the starter wire.

1. Remove the clutch release cylinder.

1. Remove the nut, bolt, ground cable and starter.