GSIC - Global Service Information Center

# STARTER > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE FRONT FENDER SEAL

1. Remove the 5 clips and seal.

3. REMOVE STARTER ASSEMBLY

1. Disconnect the starter connector.

1. Remove the nut and disconnect the starter wire.

1. Remove the 2 bolts and starter.