GSIC - Global Service Information Center

# REAR PROPELLER SHAFT ASSEMBLY > REMOVAL

## for Preparation Click here

1. REMOVE PROPELLER SHAFT WITH CENTER BEARING ASSEMBLY (for 2WD)

1. Place matchmarks on the propeller shaft flange and differential flange.

1. Remove the 4 nuts, 4 bolts and 4 washers, and disconnect the propeller shaft.

1. Remove the center support bearing's 2 set bolts and 2 plates from the frame crossmember.

1. Pull out the propeller shaft.

1. Install SST in the transmission to prevent oil leakage.

   SST
     09325-40010

2. REMOVE PROPELLER SHAFT WITH CENTER BEARING ASSEMBLY (for 4WD)

1. Place matchmarks on the propeller shaft flange and transfer flange.

1. Remove the 4 nuts, 4 bolts and 4 washers, and disconnect the propeller shaft.

1. Place matchmarks on the propeller shaft flange and differential flange.

1. Remove the 4 nuts, 4 bolts and 4 washers.

1. Remove the center support bearing's 2 set bolts and 2 plates from the frame crossmember.

1. Remove the propeller shaft.