GSIC - Global Service Information Center

# KNOCK SENSOR > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE ENGINE ASSEMBLY

1. Remove the engine assembly (Click here).

3. REMOVE CYLINDER HEAD SUB-ASSEMBLY

1. Remove the cylinder head (Click here).

4. REMOVE KNOCK SENSOR

1. Disconnect the sensor connector.

1. Remove the bolt and sensor.