GSIC - Global Service Information Center

### ENGINE OIL COOLER > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE NO. 1 ENGINE UNDER COVER (for 4WD)

3. REMOVE NO. 2 ENGINE UNDER COVER (for 4WD)

4. DRAIN ENGINE OIL

5. LOOSEN FUEL TANK ASSEMBLY

6. DRAIN FUEL

7. REMOVE MANIFOLD STAY

8. REMOVE OIL LEVEL GAUGE SUB-ASSEMBLY

9. REMOVE FUEL INLET PIPE SUB-ASSEMBLY

10. REMOVE INJECTION PIPE

11. REMOVE OIL FILTER SUB-ASSEMBLY

12. REMOVE STARTER ASSEMBLY

13. REMOVE FUEL SUPPLY PUMP ASSEMBLY

14. REMOVE COMMON RAIL ASSEMBLY

15. REMOVE OIL COOLER COVER SUB-ASSEMBLY

16. REMOVE OIL COOLER ASSEMBLY