GSIC - Global Service Information Center

# ACCELERATOR PEDAL ROD > INSTALLATION

## for Preparation Click here

1. INSTALL ACCELERATOR PEDAL ROD ASSEMBLY

1. Install the pedal rod with the 2 bolts.

   Torque:
     5.0 N*m{ 51 kgf*cm , 44 in.*lbf }

1. Connect the accelerator position sensor connector.

2. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

3. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.