GSIC - Global Service Information Center

# 2TR-FE ENGINE MECHANICAL > TORQUE SPECIFICATIONS

Part tightened | N*m | kgf*cm | ft.*lbf
Camshaft x Camshaft timing gear | 78 | 795 | 59
Camshaft bearing cap x Cylinder head : for bolt A | 12 | 122 | 9
Camshaft bearing cap x Cylinder head : for except bolt A | 15.5 | 158 | 11
Timing gear case plug x Timing chain cover | 16.6 | 169 | 12
Timing chain guide x Cylinder head | 10 | 102 | 7
Cylinder head cover x Cylinder head | 9.0 | 92 | 80 in.*lbf
Ignition coil x Cylinder head cover | 9.0 | 92 | 80 in.*lbf
Engine mounting bracket LH x Cylinder block | 51 | 520 | 38
Engine mounting bracket RH x Cylinder block | 51 | 520 | 38
Camshaft position sensor x Cylinder head | 8.5 | 87 | 75 in.*lbf
No. 1 water by-pass pipe x Timing chain cover | 17.5 | 179 | 13
V-ribbed belt tensioner x Timing chain cover : for bolt 1 | 40 | 408 | 30
V-ribbed belt tensioner x Timing chain cover : for bolt 1 | 40 | 408 | 30
V-ribbed belt tensioner x Timing chain cover : for bolt 2 | 21 | 214 | 15
V-ribbed belt tensioner x Timing chain cover : for bolt 3 | 43 | 438 | 32
Compressor mounting bracket x Cylinder block : for bolt A and B | 45 | 459 | 33
Compressor mounting bracket x Cylinder block : for bolt C | 24.5 | 250 | 18
Exhaust manifold x Cylinder head | 36 | 367 | 27
Air switching valve x Cylinder head | 20 | 204 | 15
Intake pipe insulator x Air switching valve | 20 | 204 | 15
Intake pipe insulator x Exhaust manifold | 20 | 204 | 15
Exhaust heat insulator x Exhaust manifold | 12 | 122 | 9
Intake manifold x Cylinder head | 25 | 255 | 18
Ground wire x Cylinder block | 31 | 316 | 23
Ventilation pipe x Cylinder head cover | 18 | 184 | 13
Engine mounting bracket x Body | 38 | 388 | 28
Rear end plate x Cylinder block | 18 | 184 | 13
Flywheel x Crankshaft | 1st: 26.5 2nd: Turn 90° | 1st: 270 2nd: Turn 90° | 1st: 20 2nd: Turn 90°
Cooler compressor x Compressor mounting bracket | 25 | 255 | 18
Suction hose x Timing chain cover | 5.4 | 55 | 48 in.*lbf
Oil dipstick guide x Cylinder head | 8.0 | 82 | 15 in.*lbf
Vane pump x Timing chain cover | 25 | 255 | 18
Engine wire x Junction block | 13 | 133 | 10
Ground wire x Cylinder block | 31 | 316 | 23
Ground wire x Body | 13 | 133 | 10
A/F sensor bracket x Body | 13 | 133 | 10
Air cleaner x Body | 14 | 143 | 10
Intake air connector x Cylinder head cover | 8.0 | 82 | 71 in.*lbf
Intake air connector x Hose clamp | 5.0 | 51 | 44 in.*lbf
No. 1 engine under cover x Body | 28 | 286 | 21
Side cover RH x Body | 28 | 286 | 21
Side cover LH x Body | 28 | 286 | 21
Camshaft bearing cap x Cylinder head : for bolt A | 12 | 122 | 9
Camshaft bearing cap x Cylinder head : for except bolt A | 15.5 | 158 | 11
Stud bolt x Cylinder block | 7.5 | 77 | 66 in.*lbf
No. 2 balance shaft drive gear x Balance shaft | 36 | 365 | 26
No. 2 balance shaft thrust washer x Cylinder block | 18 | 184 | 13
No. 1 balance shaft drive gear x Balance shaft | 36 | 365 | 26
No. 1 balance shaft thrust washer x Cylinder block | 18 | 184 | 13
Oil nozzle x Cylinder block | 7.0 | 71 | 62 in.*lbf
Water drain cook x Cylinder block | 25 | 250 | 18
Water drain cook plug x Water drain cook | 13 | 130 | 9
Crankshaft bearing cap x Cylinder block | 1st: 39 2nd: Turn 90° | 1st: 398 2nd: Turn 90° | 1st: 29 2nd: Turn 90°
Connecting rod cap x Connecting rod cap | 1st: 24.5 2nd: Turn 90° | 1st: 250 2nd: Turn 90° | 1st: 18 2nd: Turn 90°
No. 1 head straight screw plug x Cylinder head | 44 | 449 | 32
No. 2 head straight screw plug x Cylinder head | 90 | 918 | 66
Stud bolt x Cylinder head : for A | 3.0 | 31 | 27 in.*lbf
Stud bolt x Cylinder head : for B and C | 7.5 | 76 | 66 in.*lbf
Oil control valve filter plug x Cylinder head | 30 | 306 | 22
No. 4 chain vibration damper x Cylinder block | 18 | 185 | 13
Balance shaft drive gear shaft x Cylinder block | 25 | 255 | 18
No. 2 chain tensioner x Cylinder block | 18 | 185 | 13
No. 3 chain vibration damper x Cylinder block | 18 | 185 | 13
No. 2 chain vibration damper x Cylinder block | 27 | 270 | 20
Rear oil seal retainer x Cylinder block | 13 | 133 | 10
Oil filter bracket x Cylinder block : for union bolt | 24.5 | 250 | 18
Oil filter bracket x Cylinder block : for nut | 25 | 255 | 18
Oil filter union x Cylinder block | 43.1 | 440 | 32
Oil filter x Oil filter bracket | 17.2 | 175 | 13
Cylinder block x Cylinder head | 1st: 39 2nd: Turn 90° | 1st: 398 2nd: Turn 90° | 1st: 29 2nd: Turn 90°
Camshaft timing sprocket x Camshaft | 78 | 795 | 59
Chain vibration damper x Cylinder block | 21 | 214 | 15
Chain tensioner slipper x Cylinder block | 21 | 214 | 15
Chain tensioner x Cylinder block | 10 | 102 | 7
Oil pump relief valve x Timing chain cover | 49 | 500 | 36
Water pump x Timing chain cover | 9.0 | 92 | 80 in.*lbf
Timing chain cover plug x Timing chain cover | 16.6 | 169 | 12
Timing chain cover x Cylinder block : Excluding bolt A, tighten the bolts and nuts in this order: Area 1, Area 2, Area 3 | 21 | 214 | 15
Timing chain cover x Cylinder block : Tighten the bolts labeled A in this order: Area 2 and Area 3: | 46 | 469 | 34
Timing chain cover x Cylinder block : Tighten the bolts labeled E for Area 4 | 21 | 214 | 15
Stud bolt x No. 1 oil pan : for A | 7.5 | 76 | 66 in.*lbf
Stud bolt x No. 1 oil pan : for B | 3.0 | 31 | 27 in.*lbf
No. 1 oil pan x Cylinder block | 26 | 265 | 19
Oil strainer x No. 1 oil pan | 20 | 204 | 15
No. 2 oil pan x No. 1 oil pan | 9.0 | 92 | 81 in.*lbf
Crankshaft x Crankshaft pulley | 260 | 2,651 | 192
Ventilation valve x Cylinder head cover | 5.0 | 51 | 44 in.*lbf